(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 80)
    (zones 0)
    (modules 24)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2032)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 GND)
  (net 5 +8V)
  (net 6 "Net-(D7-Pad2)")
  (net 7 "Net-(Q1-Pad1)")
  (net 8 EN1)
  (net 9 FBLANK)
  (net 10 ~EN2)
  (net 11 "Net-(R2-Pad1)")
  (net 12 "Net-(R3-Pad2)")
  (net 13 "Net-(R4-Pad2)")
  (net 14 "Net-(R5-Pad2)")
  (net 15 ROUT)
  (net 16 GOUT)
  (net 17 BOUT)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.2032)
    (add_net +8V)
    (add_net BOUT)
    (add_net EN1)
    (add_net FBLANK)
    (add_net GND)
    (add_net GOUT)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net ROUT)
    (add_net ~EN2)
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 91.694 77.724)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.524) (layer B.SilkS))
    (fp_text value 1uF (at 0 1.524) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +8V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 64.77 77.47 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -2.794 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +8V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 66.04 67.31 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 75 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 96.52 75.692)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 0.508 1.778) (layer B.SilkS))
    (fp_text value 1N4148WS (at 0.254 -5.08 90) (layer B.Fab))
    (fp_text user %R (at 0 1.85) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 ROUT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_DIP_SPSTx04_Piano_10.8x11.72mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 5A4E1405)
    (at 123.952 65.278 270)
    (descr "4x-dip-switch SPST , Piano, row spacing 7.62 mm (300 mils), body size 10.8x11.72mm")
    (tags "DIP Switch SPST Piano 7.62mm 300mil")
    (fp_text reference SW1 (at 10.414 5.08 180) (layer F.SilkS))
    (fp_text value SW_DIP_x04 (at 7.112 3.81 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +8V))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx04_Piano_10.8x11.72mm_W7.62mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-11A_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 83.82 82.296)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-11A example for new part number: 22-27-2111, 11 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J4 (at 7.62 -4.064) (layer F.SilkS))
    (fp_text value Conn_01x11_Male (at 12.954 1.524) (layer F.Fab))
    (fp_text user %R (at 12.954 0) (layer F.Fab))
    (pad 11 thru_hole oval (at 25.4 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 FBLANK))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 EN1))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 ~EN2))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +8V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 ROUT))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 GOUT))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 17 BOUT))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-11A_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 91.186 67.564 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.524 90) (layer B.SilkS))
    (fp_text value 75 (at 2.794 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 110.49 75.692)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 1.524) (layer B.SilkS))
    (fp_text value 75 (at 0 1.524) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 123.19 75.184 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.667 0) (layer B.SilkS))
    (fp_text value 2.7k (at 0 1.524 180) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 120.65 77.978 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.794 0 90) (layer B.SilkS))
    (fp_text value 10k (at 3.302 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 ~EN2))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 117.856 76.2 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.54 0 180) (layer B.SilkS))
    (fp_text value MMBT3904 (at 2.54 -0.762 180) (layer B.Fab))
    (fp_text user %R (at -0.08 0 180) (layer B.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 53.848 75.692)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J3 (at -6.096 3.81) (layer F.SilkS))
    (fp_text value B (at 0 -1.524 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 79.248 75.692)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J2 (at -5.334 3.556) (layer F.SilkS))
    (fp_text value G (at 0 -1.524 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 104.648 75.692)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J1 (at 8.89 0) (layer F.SilkS))
    (fp_text value R (at 0 -1.524 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 122.428 77.978 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at -2.794 0 90) (layer B.SilkS))
    (fp_text value 1N4148WS (at -8.89 0 90) (layer B.Fab))
    (fp_text user %R (at -2.794 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 EN1))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 124.46 77.978 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at -2.794 0 270) (layer B.SilkS))
    (fp_text value 1N4148WS (at -8.89 0 270) (layer B.Fab))
    (fp_text user %R (at -2.794 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 FBLANK))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 61.214 75.692 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at 0 -2.032 180) (layer B.SilkS))
    (fp_text value 1N4148WS (at 5.842 0) (layer B.Fab))
    (fp_text user %R (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 17 BOUT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 64.516 75.692 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at -2.794 0 180) (layer B.SilkS))
    (fp_text value 1N4148WS (at -5.842 0) (layer B.Fab))
    (fp_text user %R (at 0 1.778 180) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 17 BOUT))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +8V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 93.218 75.692)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 1.27 1.778 180) (layer B.SilkS))
    (fp_text value 1N4148WS (at 0.762 -5.08 270) (layer B.Fab))
    (fp_text user %R (at 1.27 1.778 180) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 ROUT))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +8V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 86.614 75.692 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0.762 -1.778 180) (layer B.SilkS))
    (fp_text value 1N4148WS (at 0 5.08 270) (layer B.Fab))
    (fp_text user %R (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 16 GOUT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 89.916 75.692 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 1.016 -1.778) (layer B.SilkS))
    (fp_text value 1N4148WS (at 0.254 5.08 270) (layer B.Fab))
    (fp_text user %R (at 1.016 -1.778) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 16 GOUT))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +8V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5AE50EF0)
    (at 63.5 68.326 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C3 (at -2.667 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 7.112 -0.508 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 BOUT))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5AE50EF0)
    (at 88.9 68.326 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C2 (at -2.667 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 7.366 -0.508 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 GOUT))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5AE50EF0)
    (at 94.996 68.326 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C1 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 7.366 0.508 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 ROUT))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 25.4 (width 0.15) (layer F.Fab)
    (gr_text "1.0000 in" (at 66.548 37.308) (layer F.Fab))
    (feature1 (pts (xy 79.248 76.2) (xy 79.248 38.021579)))
    (feature2 (pts (xy 53.848 76.2) (xy 53.848 38.021579)))
    (crossbar (pts (xy 53.848 38.608) (xy 79.248 38.608)))
    (arrow1a (pts (xy 79.248 38.608) (xy 78.121496 39.194421)))
    (arrow1b (pts (xy 79.248 38.608) (xy 78.121496 38.021579)))
    (arrow2a (pts (xy 53.848 38.608) (xy 54.974504 39.194421)))
    (arrow2b (pts (xy 53.848 38.608) (xy 54.974504 38.021579)))
  )
  (dimension 22.86 (width 0.15) (layer F.Fab)
    (gr_text "0.9000 in" (at 143.54 74.93 270) (layer F.Fab))
    (feature1 (pts (xy 127 86.36) (xy 142.826421 86.36)))
    (feature2 (pts (xy 127 63.5) (xy 142.826421 63.5)))
    (crossbar (pts (xy 142.24 63.5) (xy 142.24 86.36)))
    (arrow1a (pts (xy 142.24 86.36) (xy 141.653579 85.233496)))
    (arrow1b (pts (xy 142.24 86.36) (xy 142.826421 85.233496)))
    (arrow2a (pts (xy 142.24 63.5) (xy 141.653579 64.626504)))
    (arrow2b (pts (xy 142.24 63.5) (xy 142.826421 64.626504)))
  )
  (dimension 81.28 (width 0.15) (layer F.Fab)
    (gr_text "3.2000 in" (at 86.36 29.434) (layer F.Fab))
    (feature1 (pts (xy 127 63.5) (xy 127 30.147579)))
    (feature2 (pts (xy 45.72 63.5) (xy 45.72 30.147579)))
    (crossbar (pts (xy 45.72 30.734) (xy 127 30.734)))
    (arrow1a (pts (xy 127 30.734) (xy 125.873496 31.320421)))
    (arrow1b (pts (xy 127 30.734) (xy 125.873496 30.147579)))
    (arrow2a (pts (xy 45.72 30.734) (xy 46.846504 31.320421)))
    (arrow2b (pts (xy 45.72 30.734) (xy 46.846504 30.147579)))
  )
  (gr_text "GE INTERLOGIX MVC-21S/SANYO VMC-8621P\nRGB MOD BOARD\nHTTP://WWW.DMS-100.NET" (at 64.008 82.804) (layer F.SilkS))
  (gr_line (start 45.72 86.36) (end 45.72 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 86.36) (end 45.72 86.36) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 63.5) (end 127 86.36) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 45.72 63.5) (end 127 63.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.238 85.598) (xy 46.482 85.598) (xy 46.482 64.262) (xy 126.238 64.262)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.238 85.598) (xy 46.482 85.598) (xy 46.482 64.262) (xy 126.238 64.262)
      )
    )
  )
)
